제 1차 창의작품 만들기

팀    명 : 봄이 좋냐?

학번 이름 :201634256 황예솔 201634212 김유진

작품 이름 : 종이꽃 엔딩

작품 설명 : 5년 동안 봄에 중심적인 음악은 벚꽃엔딩이었다. 계속 꾸준히 봄이 오면 차트를 점령하는 벚꽃엔딩을 표현하기 위해 벚꽃은 아니지만 종이꽃으로 대체하여 봄을 표현하고자 하였다.//[만든 목적] 팀명의 이름처럼 ‘봄이 좋냐?’이다. 봄은 제나 꾸준히 온다. 꼭 둘이 걸어야할 필요가 있을까? 라는 의문을 가지고 아두이노를 봄에 적용시켰다.

활용 가치 : 강의실 안에서도 봄에 대한 정취를 느낄 수 있으며 조도센서를 이용하여 차례로 켜지는 것을 볼 수 있으며 조도센서에 대한 이해를 할 수 있다. 뿐만 아니라 삼색 LED를 통해 초록색

아쉬웠던 점 : 삼색LED를 더 많이 활용할 수 있었다면 좋았겠지만, 브레드보드의 사이즈의 한계로 더 화려한 색을 내지 못한 것이 유감스럽다.

벚꽃엔딩을 BGM으로 넣고 싶었으나 소리가 작아 넣지 못한 것이 아쉬웠다.

스케치 파일 복사 : 황예솔 part.

void setup() {

pinMode(8, OUTPUT);

pinMode(9, OUTPUT);

pinMode(10, OUTPUT);

}

void loop() {

if(analogRead(A0)<500){

digitalWrite(8, HIGH);

digitalWrite(9, HIGH);

digitalWrite(10, HIGH);

delay(500);

}else if(analogRead(A0)<600){

digitalWrite(8, LOW);

digitalWrite(9, HIGH);

digitalWrite(10, HIGH);

}else if(analogRead(A0)<700){

digitalWrite(8, LOW);

digitalWrite(9, LOW);

digitalWrite(10, HIGH);

}else{

digitalWrite(8, LOW);

digitalWrite(9, LOW);

digitalWrite(10, LOW);

}

}

김유진 part.

void setup() {

pinMode(8,OUTPUT);

pinMode(9,OUTPUT);

pinMode(10,OUTPUT);

pinMode(11,OUTPUT);

pinMode(13,INPUT);

}

void loop() {

analogWrite(8,255);

delay(1000);

analogWrite(8,0);

delay(1000);

analogWrite(9,255);

delay(1000);

analogWrite(9,0);

delay(1000);

analogWrite(10,255);

delay(1000);

analogWrite(10,0);

delay(1000);

analogWrite(8,255);

analogWrite(9,255);

analogWrite(10,255);

delay(1000);

analogWrite(8,0);

analogWrite(9,0);

analogWrite(10,0);

delay(1000);

int value= digitalRead(13);

if (value==HIGH){

digitalWrite(11,HIGH);

}else {

digitalWrite(11,LOW);

}

}

완성작품 이미지컷 :